CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.4/conf/instr/spect/uxnmr.info
Date         : Mon Jul 31 19:09:13 2023
Release      : TopSpin 3.6.4
Installed in : /opt/topspin3.6.4
Host         : CZC7378Y6R
OS           : CentOS Linux release 7.6.1810 (Core) 
CPU          : Intel(R) Xeon(R) CPU E5-1620 v4 @ 3.50GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III 800 NMR spectrometer
1H-frequency : 800.21 MHz
Description  : Avance III
Location     : CBMR 800MHz Lab, Lucknow
Bruker Order : ZH053108
Configured in: CZC7378Y6R:/opt/topspin3.6.4/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.97
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/01554 ECL 05.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2
DRU2: AQS DRU-E Z102520/01555 ECL 05.00
- TCP/IP address = 149.236.99.88
- Firmware Version = 170619

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x4    AW  R  4.4 REC-1  AQS RXAD1000 Z102118/209 ECL 04.04
     3   0x34 0xc1   0x1        X  2.2 REF-1  REF-1000 Reference Board for AQS Receiver
     4   0x24 0x29   0x8    AE  S  3.4 SGU-1  AQS SGU/2 1000 Z103082/00524 ECL 03.04 FPGA-Vs=AF
     6   0x11 0x52   0x4    AW  R  4.4 REC-2  AQS RXAD1000 Z102118/210 ECL 04.04
     7   0x25 0x29   0x8    AE  S  3.4 SGU-2  AQS SGU/2 1000 Z103082/00523 ECL 03.04 FPGA-Vs=AF
     8   0x26 0x29   0x8    AE  S  3.4 SGU-3  AQS SGU/2 1000 Z103082/00526 ECL 03.04 FPGA-Vs=AF
     9   0x27 0x29   0x8    AE  S  3.4 SGU-4  AQS SGU/2 1000 Z103082/00528 ECL 03.04 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0262 W1345093/0262 ECL 1:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0262 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0862 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00725 ECL 03
BLA_W1345093_0261 W1345093/0261 ECL 1:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0261 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0863 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00795 ECL 03
BLA_W1345097_0120 W1345097/0120 ECL 1:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0120 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0660 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00797 ECL 03

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210212
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- 2HTX Amplifier: not available
- Lock: installed

Cryo Controller CRCO: device connected to 149.236.99.97:/dev/tty04

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.97:/dev/tty01

Eurotherm VTU: device connected to 149.236.99.97:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003465, SN=00123 from 20090128
    Module  2 : 2H
                PN=Z003476, SN=00127 from 20090709
    Module  3 : 13C
                PN=Z003527, SN=00099 from 20081030
    Module  4 : 15N
                PN=Z003533, SN=00095 from 20080707
    Module  5 : XBB31P 2HS
                PN=Z003509, SN=00147 from 20080709



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0120 at TCP/IP 149.236.99.92)
SGU1 AUX  output -> TUNE signal input of HPPR
SGU2 NORM output -> input 2 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0120 at TCP/IP 149.236.99.92)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0261 at TCP/IP 149.236.99.93)
SGU3 AUX  output -> input 3 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0120 at TCP/IP 149.236.99.92)
SGU4 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0262 at TCP/IP 149.236.99.94)
SGU4 AUX  output -> input 4 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0120 at TCP/IP 149.236.99.92)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0262 at TCP/IP 149.236.99.94:
- amplifier X-500W uses blanking 4

transmitter 2 = BLAX500 E 6-365MHZ INR W1345093/0261 at TCP/IP 149.236.99.93:
- amplifier X-500W uses blanking 3

transmitter 3 = BLAXH2H500/100/250 E 700-900MHZ  W1345097/0120 at TCP/IP 149.236.99.92:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking


